ANNEX B – PRICING SCHEDULE
Five-Year Lloyds Docking Survey Tugs: Powerful & Faithful
RFP No.: MPS-DD-2026-001
This Appendix forms part of the Request for Proposals and is to be completed and submitted by each Proponent. Pricing is to be provided separately for each vessel, Powerful and Faithful, to facilitate a like-for-like evaluation. Unless expressly stated otherwise below, each unit price is a price per vessel.
1. Instructions for Pricing
All prices shall be quoted in Bermuda dollars (BMD). Applicable duties and taxes shall be identified separately.
Prices shall be all-inclusive of labour, materials, equipment, subcontractors, travel, carriage, insurance, delivery, installation/set-up, testing, commissioning, project management, overhead and other costs necessary to complete the applicable Deliverable.
The Proponent shall provide a separate price for Powerful and a separate price for Faithful for each line item identified in the Pricing Schedule.
Where a Deliverable is not applicable to a particular vessel, the Proponent shall clearly state “N/A” and provide an explanation.
Approved variations, additional repairs and replacement of major components that are outside the defined Scope of Work shall not be included in the base price unless expressly identified in the Proponent’s pricing submission. Such work shall be subject to the applicable Contract variation provisions and prior written approval.
The acceptance criteria below are material requirements of the Deliverables and are provided to ensure that Proponents can price and assess the work on a consistent basis.
2. Pricing Schedule
	No.
	Deliverable / Pricing Item
	Unit of Measure
	Powerful – Unit Price (BMD)
	Faithful – Unit Price (BMD)
	Acceptance Criteria / Basis of Acceptance

	1
	Dry Docking and Docking of Vessel
	Per vessel
	
	
	Vessel successfully dry docked and secured without incident; docking arrangement accepted by the Owner’s Representative; vessel made available for Lloyd’s Register inspection.

	2
	Completion of all Lloyd’s Register and statutory survey requirements
	Per vessel
	
	
	All scheduled class and statutory surveys completed; Lloyd’s Register and applicable statutory authorities confirm required inspections have been carried out; deficiencies are documented and addressed in accordance with the Scope of Work and Contract.

	3
	Hull cleaning, blasting, inspection, repairs, coating application and preservation
	Per vessel
	
	
	Hull cleaning, surface preparation, inspections, repairs, coating and preservation completed to the specified standard; inspection records accepted by the Owner and Lloyd’s Register; no outstanding coating or hull defects affecting class approval.

	4
	Inspection, overhaul, testing and reinstallation of azimuth thrusters and associated propulsion systems, as required
	Per vessel
	
	
	Thrusters and associated propulsion systems reinstalled and operational; required overhaul, testing and commissioning successfully completed; work accepted by the Owner’s Representative and Lloyd’s Register, with no defects preventing operational service.

	5
	Inspection, servicing, testing and repair of machinery, auxiliary systems, electrical systems, tanks and underwater fittings in accordance with class requirements
	Per vessel
	
	
	Required systems inspected, serviced/repaired and tested; commissioning completed satisfactorily; systems demonstrate proper operation and work is accepted by the Owner’s Representative and Lloyd’s Register.

	6
	Inspection and certification of life saving appliances (LSA), Fire Fighting Appliances (FFA), and other statutory equipment by approved service providers
	Per vessel
	
	
	Required statutory equipment inspected, serviced and certified by approved service providers; applicable certificates are valid and accepted by Lloyd’s Register and/or the applicable Flag Administration.

	7
	Completion of dock trials, harbour trials and sea trials where required
	Per vessel
	
	
	All required trials successfully completed; propulsion, steering, electrical, alarm, safety and auxiliary systems operate satisfactorily; any remaining punch-list items are minor and do not affect safety, statutory compliance, class or operational readiness.

	8
	Submission of all inspection, testing and repair reports and supporting records
	Per vessel
	
	
	Complete documentation submitted in the required format, including applicable inspection, testing, repair, commissioning, NDT, material and trial records; documentation accepted by the Owner’s Representative.

	9
	Update of Lloyd’s Register Class Certificates and statutory certificates
	Per vessel
	
	
	All required class and statutory certificates/endorsements are issued following completion of the survey and corrective actions, without conditions preventing vessel operation, and are accepted by the Owner.

	10
	Completion of all approved repairs and corrective works identified during the docking survey, including approved variations
	Per vessel / variation
	
	
	All approved repairs and corrective works completed to the satisfaction of the Owner and Lloyd’s Register. Work outside the defined Scope of Work shall be undertaken only in accordance with the Contract’s variation provisions and required written authorization, except where immediate action is necessary for safety or preservation.

	11
	Complete project close-out documentation
	Per vessel
	
	
	Complete close-out dossier submitted and accepted, including warranties, manufacturer guarantees, as-built repair records, material traceability certificates, coating documentation, OEM reports, inspection records and statutory certificates.

	12
	Redelivery of vessel
	Per vessel
	
	
	Vessel accepted by the Owner’s Representative; required class and statutory certification maintained; vessel redelivered safe, clean and fully operational, with no outstanding critical deficiencies or safety issues.



3. Pricing Summary
	
	Powerful
	Faithful
	Combined Total

	Base Pricing Total
	
	
	

	Applicable Taxes / Duties
	
	
	

	Grand Total
	
	
	


Note: The Combined Total is provided for evaluation convenience only. The Proponent must maintain separate vessel pricing for Powerful and Faithful throughout its submission.
4. Schedule of Rates for Additional Works
Proponents shall provide the following schedule of rates for potential additional works that may be required outside the defined Scope of Work. These rates will be considered as part of the procurement and contract negotiation process and may be used as the basis for pricing approved variations or additional works identified during the execution of the Services.
Submission of these rates does not constitute authorization to undertake additional work or a commitment by the Government to purchase any additional services. All additional work shall remain subject to the applicable Contract variation provisions and prior written approval by the Government.
	No.
	Description
	Unit
	Rate (BMD)

	1
	Project Manager / Superintendent
	Per hour
	

	2
	Naval Architect / Marine Engineer
	Per hour
	

	3
	Mechanical Technician / Fitter
	Per hour
	

	4
	Electrical Technician / Electrician
	Per hour
	

	5
	Welder / Fabricator
	Per hour
	

	6
	General Shipyard Labour
	Per hour
	

	7
	Crane Services
	Per hour
	

	8
	Forklift / Material Handling Equipment
	Per hour
	

	9
	Additional Dry Dock Occupancy
	Per day
	

	10
	Additional Berth / Quayside Occupancy
	Per day
	

	11
	High-Pressure Washing
	Per hour
	

	12
	Grit Blasting / Surface Preparation
	Per square metre
	

	13
	Steel Renewal - Labour
	Per hour
	

	14
	Steel Plate / Structural Steel
	Per kilogram
	

	15
	NDT Services
	Per hour
	

	16
	Ultrasonic Thickness Measurement (UTM)
	Per hour
	

	17
	Painting / Coating Application - Labour
	Per hour
	

	18
	Additional Sea / Harbour Trial Support
	Per hour
	

	19
	Other Specialist Labour - Specify
	Per hour
	

	20
	Other - Specify
	
	


All rates shall be quoted in Bermuda Dollars (BMD) and shall clearly identify any applicable taxes, duties, overtime premiums, minimum charges, mobilization charges, or other conditions applicable to the stated rates.
Where materials, replacement parts, specialist subcontractors, or other third-party services are required for an approved variation and cannot reasonably be priced using the rates above, the Proponent shall identify its proposed percentage mark-up, if any, applicable to such costs:
Materials / Replacement Parts Mark-up: ________ %
Specialist Subcontractor / Third-Party Services Mark-up: ________ %
The Government reserves the right to negotiate the submitted rates and mark-ups prior to Contract Award. Any additional work undertaken during the Contract shall require the Government's prior written authorization in accordance with the Contract variation provisions.
5. Proponent Confirmation
The Proponent confirms that the prices submitted above are based on the Scope of Work, Material Disclosures, Deliverables and acceptance criteria contained in the RFP and this Appendix. The Proponent further confirms that the pricing clearly identifies the cost applicable to each vessel and that any exclusions or assumptions are expressly identified in its proposal.
	Proponent Legal Name
	

	Authorized Representative
	

	Signature
	

	Date
	



End of Appendix C – Pricing Schedule
